,Width##LENGTH##INCHES,Length##LENGTH##INCHES,Height##LENGTH##INCHES,Model##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Input Power Connection##ELECTRICAL_CURRENT##AMPERES,Input Current##ELECTRICAL_CURRENT##AMPERES,Power Factor##OTHER##,Number of Poles##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,EMC Compliance##OTHER##,Enclosure Rating##OTHER##,Grounf Fault Detection##OTHER##,Local Area Network##OTHER##,Manufacturer##OTHER##,Maximum Charging Stations per 802.11 Radio Group##OTHER##,Non-Operating Humidity##OTHER##,Non-Operating Temperature##OTHER##,Open Safety Grond Detection##OTHER##,Operating Humidity##OTHER##,Operating Temperature##OTHER##,Panel Length##LENGTH##INCHES,Plug-Out Detection##OTHER##,Power Measurement Accuracy##OTHER##,Power Report/Store Interval##OTHER##,Safety Compliance##OTHER##,Storage Temperature##OTHER##,Surge Protection##OTHER##,Terminal Block Temperature Rating##HVAC_TEMPERATURE##FAHRENHEIT,Wide Area Network##OTHER##,Description##OTHER##,URL##OTHER##,Wiring Diagrams##OTHER##,Wall Mount template-CT4000##OTHER##,Signage Templates##OTHER##,Signage Installations##OTHER##,PowerShare Instructions##OTHER##,Power Management Instructions##OTHER##,Mounting template-CT4000##OTHER##,Mounting Hardware##OTHER##,Grounding Requirements##OTHER##,Clearance Zone##OTHER##,Cable Attachment Instructions##OTHER##
6'-208v-30A,16.9,13.7,71.1,CT4021,208,40,30,0.92,2,6700,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",6' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
6'-208v-24A,16.9,13.7,71.1,CT4021,208,30,24,0.92,2,6200,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",6' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
6'-208v-16A,16.9,13.7,71.1,CT4021,208,20,16,0.92,2,3300,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",6' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
6'-240v-30A,16.9,13.7,71.1,CT4021,240,40,30,0.92,2,7700,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",6' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
6'-240v-24A,16.9,13.7,71.1,CT4021,240,30,24,0.92,2,7200,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",6' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
6'-240v-16A,16.9,13.7,71.1,CT4021,240,20,16,0.92,2,3800,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",6' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
8'-208v-30A,19,13.7,96,CT4025,208,40,30,0.92,2,6700,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",8' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
8'-208v-24A,19,13.7,96,CT4025,208,30,24,0.92,2,6200,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",8' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
8'-208v-16A,19,13.7,96,CT4025,208,20,16,0.92,2,3300,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",8' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
8'-240v-30A,19,13.7,96,CT4025,240,40,30,0.92,2,7700,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",8' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
8'-240v-24A,19,13.7,96,CT4025,240,30,24,0.92,2,7200,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",8' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf
8'-240v-16A,19,13.7,96,CT4025,240,20,16,0.92,2,3800,FCC Part 15 Class A,Type3R per UL 50E,20mA CCID with auto retry,2.4 GHz Wi-Fi (802.11 b/g/n),ChargePoint Inc.,10. Each station must be located within 150 feet “line of sight” of a gateway station.,Up to 95% @ 122°F (+50°C) non-condensing,-40°F to 140°F (-40°C to +60°C),Continuously monitors presence of safety ground connection,Up to 85% @ 122°F (+50°C) non-condensing,-22°F to 122°F (-30°C to +50°C),6.855,Power terminated per SAE J1772 specifications,+/- 2% to full scale (32A),"15 minute, aligned to hour","UL listed for USA and cUL certified for Canada; complies with UL 2594, UL 2231-1, UL 2231-2, and NEC Article 625",-22°F to 140°F (-30°C to +60°C),"6kV @ 3000A. In geographic areas subject to frequent thunder storms, supplemental surge protection at the service panel is recommended.",221,"3G GSM, 3G CDMA",8' Bollard Dual Port,www.chargepoint.com,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/75_001120_01_r1.pdf,http://www.chargepoint.com/support-guides/,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Bollard_Anchor_Bolt_Pattern_Template.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf,http://www.chargepoint.com/files/CT4000_Clear-zone.pdf,http://www.chargepoint.com/files/CT4000_Install_Guide.pdf